Lab 6 – Instructor Notes

1. Trainers used are the same ones from lab 2 and 3
2. A “high resistance short-to-ground” is created using a lamp base that has alligator clips on each end. The lamp is placed in parallel to a load (to ground). Students then have to deduct which part of the circuit has the dangerous ground, troubleshooting with their ammeter.